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PURPOSE AND SCOPE

The purpose of this procedure is to provide the steps necessary to perform the Lighting Inspection. 

FREQUENCY

The Lighting Inspection is performed twice per year or when a change to the lighting is made in the facility. 

PROCEDURE

1. Print out the Lighting Inspection form from the HACCP Forms folder in the computer. 

2. Use this diagram as you tour the facility to document the lighting lux in a variety of locations in each room. 

3. Take the calibrated handheld light meter, remove the black cover from the light meter and turn on. 

4. Rest the light meter on a flat surface when trying to take a reading. Ensure that you are not creating a shadow over the meter. Press the foot candle button a couple of times to display the proper number. 

5. When taking the light meter reading in a room without a working surface, take the reading for 1 meter off of the ground.

6. Ensure that all plant inspection sites (where CCP’s are monitored) are inspected to ensure that the lighting meets the required limits. 

7. Document the lux levels on the map of the plant. 

8. The lighting used throughout the facility is such that it does not alter food color and meets CFIA regulations as follows:

· 540 lux at all plant inspection sites 
· 110 lux in all areas where edible products are handled, and at the working surface level. 
· 110 lux in coolers, at the level of the front shank of carcasses when the room is full with carcasses, and at the lowest level of open product storage (offals).
· 220 lux in all workroom, at the working surface level
· 110 lux in all other areas of the registered establishment where there are no products


DEVIATION PROCEDURES

In the event that a light fixture is not of the appropriate lux or the lighting in an area or department is insufficient, the HACCP Team Member will document the deviation on a Maintenance Work Order Form and submit it to the Maintenance Department.

The Maintenance Department will be responsible for taking the necessary corrective actions, e.g. replacing bulbs, and documenting these on the Maintenance Work Order Form. The completed Maintenance Work Order Form will be returned to the HACCP Coordinator. 


RECORDS

Lighting Inspection Form

Disclaimer: This template is for general use only and must be customized to meet your business’s regulatory requirements
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